# How to Program Flipper Universal Remote

By: Vishnu Mohan | In: Programming | Last updated: 01/06/2025

The Flipper universal remote is a simple, big-button remote control designed for seniors, kids, and users with visual impairments. You can easily program it and configure up to 25 favorite channels for quick access, eliminating the difficulty of scrolling through unnecessary options and keeping your top shows at your fingertips.

This article will guide you through programming your flipper remote using code entry, code search, and learning methods; I will also outline steps for code retrieval and setting your favorite channels for quick access.

## Flipper Universal Remote Codes

The latest Flipper remote codes for popular TV brands are listed below:

- Haier: 3381, 3931, 3041, 1761
- Hisense: 6621, 3381, 3941, 2851, 3951
- LG: 0201, 3381, 3671, 4641, 4871, 4941
- Panasonic: 2591, 3451, 7161, 8411
- Philips: 3801, 3521, 8271, 3381, 4831
- RCA: 4001, 3591, 6641, 1721, 1791
- Samsung: 3831, 1791, 3901, 5471, 5901, 5971
- Sanyo: 4011, 4021, 1771, 3141, 3221
- Sharp: 6621, 6721, 3421, 3861
- Sony: 6391, 3611, 0141, 3391
- TCL: 3441, 4131, 1481, 3381, 4141
- Toshiba: 4051, 2861, 4181, 4061, 3601
- Vizio: 1761, 3841, 3541, 5821
- Zenith: 5301, 0461, 1761, 4541, 4871, 4891

For more brands and devices, use the code lookup tool below.

### Flipper Remote Code Lookup Tool

Remote Version

Device Type

Brand

Note: The codes are compiled from multiple sources, so not all codes may be compatible with your specific remote model.

## How to Program Flipper Universal Remote

To program the Flipper remote to your TV:

1. Press and hold the TV button until the light stays on.
2. Enter the 4-digit code for your TV brand (e.g., 6391 for Sony).
3. Test the VOLUME and CHANNEL buttons. If the code doesn’t work, repeat with the next code until it does.

Now, let’s dive into the details of programming your Flipper remote using various methods.

Note: Slide down the bottom half of the front panel to access the numeric keypad and the setup buttons before programming.

### Direct Code Entry

1. Press and hold the device button (TV, STB, or LC) until the light stays on.
2. Enter a 4-digit code for your device.
3. Test VOLUME+/- and CHANNEL+/-. If the code doesn’t work, repeat with the next code in the list.

Notes:

- Program TV and STB separately for VOLUME and CHANNEL functions.
- To pair a soundbar (available from V6 onwards), press LC in Step 1.
- To map CHANNEL buttons to your TV (if no STB and soundbar), hold TV until the light stays on, then enter ‘970‘.

If no 4-digit codes work for your brand or it isn’t listed, try the auto code search method below:

### Auto Code Search

1. Press and hold the device button (TV or STB) until the light stays on.
2. Enter the regional code: ‘962‘ for US/Canada or ‘961‘ for UK/EU/Pacific. The light will stay lit.
3. Press ON/OFF to send a batch of 15 codes. If the device doesn’t turn off, repeat until it does.
4. When the device turns off, press CHANNEL- (Channel down) slowly to send one code at a time until it turns back on.
5. Press the device button (TV or STB) to save. Test all functions to confirm.

#### Code retrieval

The code retrieval feature lets you find the working code after a successful code search. Once retrieved, you can note it for future use, allowing quick programming via direct code entry without repeating the lengthy auto code search process.

To retrieve the code:

1. Press TV (or STB), then press ‘1’ and release both. Count the flashes; this is the 1st digit.
2. Press TV (or STB), then press ‘2’ and release both. Count the flashes; this is the 2nd digit.
3. Press TV (or STB), then press ‘3’ and release both. Count the flashes; this is the 3rd digit.
4. Press TV (or STB), then press ‘4’ and release both. Count the flashes; this is the 4th digit.

Note: If there are no flashes, the digit is zero.

If the code search method doesn’t work, you can teach the remote the function directly from the original remote using the learning method described below.

### Learning Functions

Flipper can learn IR signals from your existing original remote by programming each button separately. For TV signals, use the TV button; for STB functions, use the STB button; and for soundbar functions, use the LC button. Ensure to perform this process in low light to avoid interference with the IR signal.

To learn an IR signal:

1. Place the Flipper remote and your original device remote on a table, facing each other.
2. On Flipper, press and hold the TV (or STB or LC) and ON/OFF buttons together until the light flashes, then release both buttons.
3. Press and release the key you want to copy on Flipper (e.g., VOL+). The light will stay solid. Press and release the same key on your device remote until the light flashes. When the light blinks, the remote successfully learns the key. Repeat for all desired keys.
4. Press TV (or STB or LC) to exit.
5. Test the learned keys. If any do not work as expected, repeat the process until all keys are correctly learned.

Notes:

- TV, STB, and ADD do not learn functions.
- Favorite channel mode will not work with the learning setup.

### Setting Favorites

After setting up your Flipper remote, you can program up to 25 favorite channels. Start by listing the channels you want in the order they’ll scroll. The channels will advance only in the order they are entered. For example, if you program channels 115, 155, 48, and 326, the Channel Up/Down buttons will cycle through them in that sequence only. Flipper does not automatically arrange channels in numeric order.

STBs and TVs typically use a 3 or 4-digit channel entry system, such as 000 or 0000. To enter a channel, use leading zeros as placeholders. For example, enter channel 7 as 007 (three-digit) or 0007 (four-digit). If your TV or STB requires pressing the Enter key to change channels, use one of the two channel entry formats as explained below.

Flipper offers two channel entry formats: one uses the STB’s OK/Enter signal (LC) for faster channel changes, while the other does not use LC. If a search box appears when manually entering channels (using 0-9), you need to press LC (e.g., for Xfinity or Contour). If pressing LC brings up a menu, reprogram without using LC (e.g., for some DirecTV boxes).

#### For TV and STB

1. Hold STB and ADD together until the light stays solid.
2. Add a channel by entering the channel number (e.g., 10), pressing LC, then ADD. Repeat for all desired channels.
3. Press STB to exit. The light turns off.

#### For TV Only

Set favorites in TV: On your TV remote, press the Menu button on your remote, navigate to Settings, and then Add/Delete Channels (or a similar option based on your TV model). From there, adjust your channel list by adding or removing channels as needed.

Set favorites in Flipper: On Flipper, press and hold TV and ADD simultaneously until the light turns solid. Then, enter the channels (e.g., 123), followed by pressing ADD.

Note: Some cable providers use sub-channels like 5-1 or 5.1, but many codes do not support these signals. So, try different codes until you find a match, or set favorites on the TV as described above.

#### Adjusting IR Timing

When using favorites, you need to allow the box to change channels before pressing the channel button again. Some older Xfinity boxes may need extra time to process signals due to older chips and aren’t designed for Flipper’s favorites feature.

If favorites are switching to random channels despite waiting for them to change, try slowing down the IR speed.

To decrease the speed, press and hold the device button (STB or TV) and CH- for 3 seconds until the light flashes once. This adjusts the speed by one level. After each level, test the favorites feature. Repeat the process up to 5 levels to find the optimal speed.

#### Deleting Favorites

1. Press and hold STB and DEL together until the light stays on.
2. Enter the channel number to delete, then press LC and DEL (or just DEL).

Note: It is important to delete the exact channel that was originally programmed. Keep in mind that the resulting channel may not always match what was programmed. This occurs because, if the specified channel is not in the channel lineup, the device will automatically tune to the nearest available channel instead.

### On/Off Options

Flipper is preset to turn both the TV and STB on and off by default. However, occasionally, one device may remain on while the other is off.

To modify the Flipper remote so only the TV turns on and off:

- TV Only: Press and hold ADD until the light turns solid, then enter ‘999‘. Then disable any standby or power-saving mod e on the box.
- TV and STB: Press and hold the ADD button until the light turns solid, then enter ‘998‘.
- TV, STB, and SoundBar: Press and hold ADD until the light turns solid, then enter ‘997‘.

### Volume Options

By default, Flipper controls Soundbar volume (V6 and above).

- To switch to TV volume: Press and hold ADD + VOL- for 3 seconds. The indicator will flash once and turn off.
- To switch to STB volume: Press and hold ADD + VOL+ for 3 seconds. The indicator will flash once and turn off.

### Resetting to Factory Settings

To reset the Flipper remote to its factory settings, press and hold ADD until the light flashes once and stays on. Then, enter 954, and the light will flash twice. If the older settings persist, repeat the process with both the TV and STB to confirm the reset.

In conclusion, the Flipper universal remote makes controlling your TV, setting favorite channels, and customizing settings easy and intuitive. Whether you’re using code entry, auto search, or the learning method, programming is simple and flexible. The ability to program favorite channels, adjust IR timing, and seamlessly switch between devices provides a personalized experience for every user. I hope this guide was helpful. If you have any questions or encounter issues, feel free to ask in the comments.

## FAQs

### Does Flipper remote work With Roku, Google TV, Apple TV, and Amazon?

No, the Flipper remote currently does not support streaming devices like Roku, Google TV, Apple TV, or Amazon Fire TV. However, it does support TVs with streaming integration, but only basic functions on smart TVs.

### Does Flipper remote work with sub-channels?

The Flipper Remote may not work with all TVs or digital-to-analog boxes (DTAs) that use sub-channels like 5-1 or 45.2, as these signals are relatively new. Older TVs may not be compatible with the current code set. Try different codes to find a match.

### How can I fix random channels appearing?

If random channels appear or double digits (like 44) are showing as a single digit, make sure to allow the channel to fully change before pressing the Channel button again. If the issue persists, try decreasing the timing of the IR signal.

### How to stop the guide from appearing when using favorites?

To prevent the guide from appearing, use a different Channel Entry Format when setting favorites. Avoid the LC (OK) signal; for example, use "123, ADD" instead of "123, LC." If the issue persists, delete the favorites or reset the remote to factory settings.

#### About the Author: Vishnu Mohan

Vishnu is a professional home theater technician and experienced AV installer with over 7 years of hands-on experience setting up custom home entertainment systems. He specializes in universal remote programming, system troubleshooting, and AV integration and optimization, with a focus on making complex setups intuitive and user-friendly. He has extensive experience with a wide range of brands, including Logitech Harmony, GE, RCA, One For All, and more, and enjoys helping users get the most out of their devices. When he's not on the job, he shares remote codes, programming procedures, and troubleshooting tips right here on the blog to help others confidently take control of their home tech.

### Leave a Reply Cancel reply

Your email address will not be published. Required fields are marked *

Comment *

Name *

Email *

Website

Save my name, email, and website in this browser for the next time I comment.