# How to Program Altice Optimum Remotes

By: Vishnu Mohan | In: Programming | Last updated: 01/06/2025

Altice Optimum remotes (formerly Suddenlink) include standard (such as URC2464, Maestro XL, etc.) and voice-controlled models (like Altice One and Stream remote) that come with Optimum One, Optimum TV box, and Optimum Stream box. These remotes are universal, and you can easily program them to control your TV’s volume and power functions, as well as your set-top box functions.

This article provides step-by-step programming instructions for various Optimum remote models. To simplify the process, I’ve included a code lookup tool to help you quickly find the correct codes for your device.

## Altice Optimum Remote Codes

Below are the 4-digit Optimum remote codes for major TV brands:

- Emerson: 0051, 0081, 3151, 2891, 2821, 2571
- Haier: 1131, 1191, 4141, 0341, 1661
- Hisense: 0051, 0981, 0771, 4141, 0261, 0311
- Insignia: 0271, 2311, 4141, 0991, 1751
- LG: 0051, 4111, 4141, 3301, 2851, 1661
- Panasonic: 0131, 2671, 1831, 2751, 2071
- Philips: 0181, 1311, 0001, 4141, 3811, 2421
- Samsung: 0151, 3071, 1461, 2831, 0051
- Sceptre: 0391, 0141, 3711
- TCL: 1111, 0821, 0001, 1661, 1561
- Toshiba: 0331, 2831, 0131, 0101, 3641, 2151
- Vizio: 0171, 1891, 0051, 4121

To find codes for more brands, use the code lookup tool below.

### Optimum Remote Code Lookup Tool

Remote Type

Device Type

Brand

Note: The codes are compiled from multiple sources, so not all codes may be compatible with your specific remote model.

## How to Program Altice Optimum Remotes

Optimum remotes come in different models, each with its own programming steps. To make it easier, I have unified each programming method for all remote models, clearly outlining the steps. Simply follow the instructions for your specific model to avoid any confusion.

Note: If you are unsure which remote you have, click the links to view images of the remotes.

- Altice One (Optimum One)
- Altice Maestro XL (T4HU1617 64k)
- Altice Digital Adapter Remote
- UR2-CBL-CV04 (Silver with “iO” button)
- URC2464 (Silver with “O.” button)

- Polaris URC1090
- Atlas URC1056
- Pulse Remote
- Delta URC3068
- Optimum Stream

### Direct Code Entry

1. Prepare the device:
   - Turn on your TV.
2. Activate programming mode:
   - Altice One/Digital Adapter/Maestro XL: Hold TV Power + SELECT/OK until the light blinks twice.
   - UR2-CBL-CV04: Hold TV + SEL for 3 seconds until the “iO” button lights up.
   - URC2464: Hold TV Power + SEL until the “O.” blinks twice.
   - Polaris: Hold SETUP until TV Power blinks twice.
   - Atlas: Press the mode key (e.g., TV), then hold SETUP until it blinks twice.
   - Pulse IR & RF: Hold SETUP until the LED blinks twice.
   - Delta: Hold SET until the red LED blinks twice.
3. Enter the code:
   - Most remotes: Use a 4-digit code.
   - Delta: Use a 5-digit code.
   - UR2-CBL-CV04: Use a 3-digit code.
4. Test Functions:
   - Try Power, VOL+/-, and MUTE:
     - If buttons work, setup is complete.
     - If not, repeat with another code.
   - UR2-CBL-CV04: Press MUTE to turn the TV on, then press the TV button to save the code (iO button blinks to confirm).

### Manual Code Search

1. Prepare the device:
   - Turn on your TV (or other device).
2. Enter programming mode:
   - Altice One/Maestro XL: Hold TV Power + SELECT/OK until the light blinks twice.
   - Altice Digital Adapter: Hold TV Power + VOL+ for 3 seconds until the light stays on.
   - UR2-CBL-CV04: Hold TV + SEL for 3 seconds until the “iO” button lights up.
   - URC2464: Hold TV Power + SEL until the “O.” blinks twice.
   - Polaris/Atlas/Delta: Hold SETUP (or SET for Delta) until the light blinks twice.
   - Pulse IR & RF: Hold SETUP until the LED blinks twice.
3. Search for the code:
   - Altice One/Maestro XL/URC2464/Pulse IR & RF: Hold SELECT/OK (or OK/ENTER) until the TV turns off.
   - Altice Digital Adapter: Press and release 1, then hold TV Power until the TV turns off. Press SELECT to save.
   - UR2-CBL-CV04: Press CH+ or CH- until the TV turns off.
   - Polaris/Atlas/Delta: Enter 9-9-1, then press CH+ repeatedly until the TV turns off.
4. Save the code:
   - Press the following to save the working code:
     - Altice Digital Adapter: SELECT.
     - UR2-CBL-CV04: TV (iO button blinks twice).
     - Polaris/Atlas/Delta: SETUP or SET.
5. Test the remote:
   - Verify TV Power, VOL+/-, and MUTE buttons.
   - If they don’t work, repeat the process.

### One-Digit Code Search

1. Prepare your TV:
   - Ensure your TV is powered on.
2. Activate programming mode:
   - Altice One/Digital Adapter: Hold TV Power + the number key for your brand for 3 seconds until the light turns on.
   - Maestro XL: Hold TV Power + SELECT/OK until the HOME/MENU button blinks twice, then press TV Power.
   - URC2464: Hold TV Power + SEL until the “O.” button blinks twice, then press TV Power.
   - Pulse IR & RF: Hold SETUP until the LED blinks twice, then press TV Power.
3. Enter the one-digit code:
   - Hold the number button for your TV’s brand while pointing the remote at the TV.
   - Release the button when the TV turns off (this may take a few seconds).
4. Save the code:
   - Altice One/Digital Adapter: Press SELECT to store the code. The light will turn off.
   - Maestro XL: The HOME/MENU button blinks twice automatically to confirm.
   - URC2464/Pulse IR & RF: No additional step is required; proceed to testing.
5. Test the remote:
   - Check TV Power, VOL+/-, and MUTE buttons to confirm functionality.
   - If they do not work, repeat the process.

### Programming Optimum Stream Remote

#### Pairing to Stream Box

Your remote automatically pairs with your Optimum Stream box during installation. If it becomes unpaired or you get a new remote, simply follow the pairing steps.

To pair, place the Optimum Stream box in direct view of the remote. If it’s behind a TV or in a cabinet, move it temporarily so the remote can connect. Once paired, you can move the Stream box out of sight.

1. Turn on your TV and Optimum Stream box.
2. Press Home (⌂) on the Stream remote to ensure you’re on the home screen.
3. From the home screen, select Settings.
4. Choose Device and Remote Settings > Remotes & Accessories.
5. Select Add Stream Remote.
6. Follow the on-screen instructions to pair your remote.
7. Once paired, you’ll see an on-screen confirmation.

#### Programming to Control your TV

1. Once paired to the Stream box, go to Settings and select Remotes & Accessories.
2. Select Stream Remote (connected) > Change TV Set Up.
3. Follow the on-screen instructions to program your remote.
4. You’ll see an on-screen confirmation when the remote is programmed.

So, programming your optimum remote controls is well explained in the above sections. Before programming your remote, find out the compatible remote codes for your device using the code lookup tool and note it down. This makes your task much easier. If you have any issues with the programming or have any questions, feel free to ask me in the comments.

Happy programming!

#### About the Author: Vishnu Mohan

Vishnu is a professional home theater technician and experienced AV installer with over 7 years of hands-on experience setting up custom home entertainment systems. He specializes in universal remote programming, system troubleshooting, and AV integration and optimization, with a focus on making complex setups intuitive and user-friendly. He has extensive experience with a wide range of brands, including Logitech Harmony, GE, RCA, One For All, and more, and enjoys helping users get the most out of their devices. When he's not on the job, he shares remote codes, programming procedures, and troubleshooting tips right here on the blog to help others confidently take control of their home tech.

### Leave a Reply Cancel reply

Your email address will not be published. Required fields are marked *

Comment *

Name *

Email *

Website

Save my name, email, and website in this browser for the next time I comment.