# Jumbo Universal Remote Codes and Programming Instructions

By: Vishnu Mohan | In: Programming | Last updated: 01/06/2025

If you own a Jumbo universal remote and are looking for setup codes to program it, you are in the right place. This guide provides a comprehensive list of remote codes for popular models like Innovage, iWave, Emerson, Decibel Electronics (Item No. A17G2022), Sentry (RMC10 & RMC20), Harbor Freight (Model 66687), and other generic Jumbo remotes. For added convenience, I have also created a handy code finder tool to help you quickly locate the correct code for your device.

While most of these remotes use 3-digit codes, there are a few exceptions. Models such as the Harbor Freight Tools Item 61959 and the QFX REM-115 come pre-programmed with newer 4-digit codes. To make the programming process easier, I have included step-by-step instructions for both the direct code entry method and the auto code search method.

## Jumbo Universal Remote Codes

The table below lists the 3-digit and 4-digit Jumbo remote control codes for popular TV brands.

TV Brands | 3-Digit Codes | 4-Digit Codes
--- | --- | ---
Admiral | 001, 173, 211 | 0603, 0224, 0701
Daewoo | 004, 005, 006, 009, 016 | 0614, 0002, 0502, 0611
Emerson | 004, 006, 009, 012, 014, 023 | 0002, 0502, 0006, 0115, 0506
LG | 004, 005, 009, 056, 057 | 0002, 0606, 0502, 0102, 0117
Panasonic | 003, 054, 055, 062, 070, 148 | 0718, 0416, 0007, 0618, 0807
Philips | 003, 004, 006, 008 | 0807, 0022, 0020, 0422
Samsung | 015, 104, 105, 106, 109, 172 | 0112, 0309, 0209, 0512, 0302
Sansui | 135, 136 | 0115, 0632
Sharp | 004, 009, 079, 173 | 0509, 0913, 0907
Sony | 002, 006, 071, 128 | 0414, 0902, 0801, 0708
Vizio | 702, 709 | 0709, 1702

If you want device codes for more brands and devices, use our code finder tool provided below.

### Jumbo Universal Remote Code Finder

Code Type

Device Type

Brand

Note: The codes are compiled from multiple sources, so not all codes may be compatible with your specific remote model.

## How to Program Jumbo Universal Remotes

There are two main methods to program a Jumbo universal remote: Direct Code Entry, which requires a specific device code, and Auto Code Search, which does not require any codes at all. Below, you will find clear, step-by-step instructions for setting up your Jumbo remote using both methods.

### How to Program Jumbo Universal Remote with Code

To program Jumbo universal remote with code, use the Direct Code Entry method as follows:

1. Turn on the device you want to control.
2. Press and hold the CODE SEARCH button until the red LED stays on.
3. Press the device button for the device you wish to program (e.g., TV, DVD, VCR, etc.). The LED will flash once and stay lit.
4. Enter the 3-digit code using the number buttons. If the code is valid, the red LED indicator will turn off. If it’s invalid, the LED flashes, so you need to repeat the procedure with the next code for your device.
5. Press the Power button. If the device turns off, press it again. If the device powers on and all functions work correctly, you’ve found the right code. If not, repeat the process with the next code for your brand.

Note: To program the Harbor Freight Tools Item 61959 or any Jumbo remote with a MUTE instead of a CODE SEARCH button, press and hold the device button until the red LED light turns on, then enter the 4-digit code.

### How to Program Jumbo Universal Remote without Code

To program Jumbo universal remote without code, follow the Auto Code Search method as outlined below:

1. Turn on the device you want to control (e.g., TV, DVD player, VCR).
2. Press and hold the CODE SEARCH button on your Jumbo remote until the red LED stays on, then release the button.
3. Press the device button for the device you’re programming. The LED will blink once and remain lit.
4. Press and release the POWER button repeatedly while aiming the remote at your device.
   - Wait about 2 seconds between each press to allow the device time to respond.
   - Continue this process until the device turns off. It may take several attempts to cycle through all possible codes.
5. Press the ENTER button immediately after the device turns off to save the code.
6. Press the POWER button again to turn the device back on.
   - If it powers on, the code has been successfully stored. Test other buttons (like volume, channel, or play) to ensure they work correctly. If not, repeat the process.

Notes:

- If no buttons are pressed within 12 seconds after starting the setup, the CODE SEARCH feature will automatically turn off.
- For newer models such as the Harbor Freight Tools Item 61959, QFX REM-115, or any Jumbo remote that uses the MUTE button instead of CODE SEARCH, start by holding the device button until the red LED stays on. Then, press the CH+ button repeatedly until the device turns off. Once it does, press ENTER to save the code.

  Now that you have the complete list of Jumbo universal remote codes and the programming methods, you are all set to configure your remote for devices like your TV, DVD player, cable box, and more. Give it a try and get your home entertainment system up and running. If you run into any issues with the codes or setup process, feel free to leave a comment below. I am here to help.

#### About the Author: Vishnu Mohan

Vishnu is a professional home theater technician and experienced AV installer with over 7 years of hands-on experience setting up custom home entertainment systems. He specializes in universal remote programming, system troubleshooting, and AV integration and optimization, with a focus on making complex setups intuitive and user-friendly. He has extensive experience with a wide range of brands, including Logitech Harmony, GE, RCA, One For All, and more, and enjoys helping users get the most out of their devices. When he's not on the job, he shares remote codes, programming procedures, and troubleshooting tips right here on the blog to help others confidently take control of their home tech.

### Leave a Reply Cancel reply

Your email address will not be published. Required fields are marked *

Comment *

Name *

Email *

Website

Save my name, email, and website in this browser for the next time I comment.